# NVRAM file for BCM943430WLSELG
# 2.4 GHz, 20 MHz BW mode

# The following parameter values are just placeholders, need to be updated.
manfid=0x2d0
prodid=0x0726
vendid=0x14e4
devid=0x43e2
boardtype=0x0726
boardrev=0x1101
boardnum=22
macaddr=00:90:4c:c5:12:38
sromrev=11
boardflags=0x00404201
xtalfreq=26000
nocrc=1
ag0=255
aa2g=1
ccode=CN

pa0itssit=0x20
extpagain2g=0

#PA parameters for 2.4GHz, measured at CHIP OUTPUT
pa2ga0=-168,7161,-820
AvVmid_c0=0x0,0xc8
cckpwroffset0=5

# PPR params
maxp2ga0=90
txpwrbckof=6
cckbw202gpo=0
legofdmbw202gpo=0x66111111
mcsbw202gpo=0x77711111

# OFDM IIR :
ofdmdigfilttype=18
ofdmdigfilttypebe=18
# PAPD mode:
papdmode=1
#papdvalidtest=3

il0macaddr=00:90:4c:c5:12:38
wl0id=0x431b

deadman_to=0xffffffff
# muxenab: 0x1 for UART enable, 0x2 for GPIOs, 0x8 for JTAG
muxenab=0x1
# CLDO PWM voltage settings - 0x4 - 1.1 volt
#cldo_pwm=0x4

#Out-of-band GPIO Wakeup
sd_gpout=0
sd_gpval=1
sd_gpdc=0
